**SPECIFICATIONS**

|  |  |  |
| --- | --- | --- |
| **Item** | **Quantity** | **specifications** |
| 1**.**CRO 2.Function Generator3. Solar Cell VI Characteristics.  4. optical fiber characteristics 5. LASER Measurement of wavelength using milliammeter scale as grating. | 11111 | Voltage range:5V to 50V, bandwidth: 5MHz to 100MHz, frequency response: DC to upper bandwidth limit, channel: Dual.Frequency range: up to 50MHz or higherOpen circuit voltage: 0.5V to 10 V (per cell) |